|  |  |  |  |
| --- | --- | --- | --- |
| **Date of Testing** | **Staff Who Tested** | **Results** | **Comments****(send to home office immediately for repair needs)** |
| **EXAMPLE**2/2/09 8am | J.SNOW | 3 of the 4 doors passed the test | 1 door failed to alarm or release the door |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

NFPA 7.2.1.15.1 …Door assemblies shall be inspected and tested not less than annually in accordance with 7.2.1.15.1 through 7.2.1.15.7 Written record must be kept. Testing of door assemblies shall be performed by individuals who can demonstrate knowledge and understanding of operating components of the type of door being subjected to testing. Door assemblies shall be visually inspected from both sides of the opening.